**T-525A**

**User Manual**

**图形用户界面, 应用程序

描述已自动生成**

Before operating the Monitor, please read this manual thoroughly

and retain it for future reference.

**Key Description**

屏幕上有个手机

描述已自动生成

1.Power button,

;

2. CAM: Select video between CH1/CH2/CH3；


3.Increase setting value;

4.MENU”: Short press to open the monitor’s OSD menu, return to the previous menu function setting / Toggle menu function/exit menu function setting;

5.Decrease the setting value;

6.Mode-Un-mirror Image or Mirror Image switch

**Remote control instructions**



1.POWER:Power on / off the screen

2.VIDEO SELECT：Select between CH1/CH2/CH3；

3.Increase setting value;

4.Enter the menu screen and return to the previous menu function setting / exit menu function setting/exit menu function setting;

5.Decrease the setting value;

6: Color mode adjustment, you can choose USER/DAY/NIGHT1/NIGHT2/NIGHT3.

**Specifications**

|  |  |  |
| --- | --- | --- |
| **Item** | | **parameter** |
| System language | | Chinese, English, Other (can be customized) |
| LCD | Screen Size | 5’’ |
| Video | Video input | 3 CH Video Inputs. 720P@25/30,1080P @25/30 or CVBS  PAL& NTSC Auto Recognize |
| Resolution | 800\*480 (IPS Panel) |
| Power and power consumption | Power management | Adaptive wide-format power input with protection functions such as low voltage, over voltage, and reverse short circuit; |
| Input voltage | DC: +12V ~ +36V |
| Output voltage | +12V |
| Power consumption | Normal working status <5W (without display and camera) |
| Working environment | Temperature | -30℃ ~ +70℃ |
| Humidity | 20% ~ 80% |

**Functions Description**

1.Press the MENU button to enter the **IMAGE SETTING**.

蓝色的屏幕

描述已自动生成

Using “Mode” button to choose "BRIGHTNESS” or “CONTRAST” or “SATURATION” or “RESET” settings, use button 3 or button 4 to set the value. Use button 3 or button 4 to restore default settings;

1. Press the MENU button to enter the **GENERAL SETTING**.

屏幕上有字

描述已自动生成

Using “Mode” button to choose CH1/CH2/CH3’s "GUIDES” settings, use button 3 to 4 to turn on and off it. After trigger wire is activated, the parking lines will be turned on or off.

Using “Mode” button to choose CH1/CH2/CH3’s "DELAY” settings, use button 3 to 4 to turn on (1-15 seconds settable) or off it. After correspond trigger wire is activated, the triggered displayed image will keep showing for the set period (1-15 seconds) before switching to the default image.

3. Press the MENU button to enter the **SYS SETTING**.

蓝色的屏幕

描述已自动生成

Using button 3 and button 4 to choose the languages settings— English, Russian, Japanese, Korean.

Using “Mode” button to choose the UPSIDE DOWN setting, use button 3 or button 4 to turn on or off it. If turn it on, you can install the monitor’s U bracket to the ceiling of your vehicle.

Using “Mode” button to choose MIRROR setting, use button 3 or button 4 to turn on or off the mirrored or un-mirrored function.

**Wiring Diagram**

图片包含 日程表

描述已自动生成